{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet3"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet3","index":0,"n_rows":30,"n_cols":3,"rows_kept":30}
["Company","Delta","Delta"]
["Series","MS300","ME300"]
["Power Range 1ph 220V","100W- 2.2KW","100W- 2.2KW"]
["Power Range 3ph 400V","400W-22KW","400W-7.5KW"]
["Max output Freq",599,599]
["ND OL","120% for 1 min, 150% for 3 sec every  Minutes","120% for 1 min, 150% for 3 sec every  Minutes"]
["HD OL","150% for 1 min, 200% for 3 sec every  Minutes","150% for 1 min, 200% for 3 sec every  Minutes"]
["Digital Input",7,5]
["Analog Input",2,1]
["Analog Input Voltage","-10V to 10V","0 to 10V"]
["Pulse Input","1 (33KHz)","1 (33KHz)"]
["Analog Output",1,1]
["Digital Output","2 + Pulse Output",1]
["Relay output",1,1]
["Keypad ","Analog potentiometer","Analog potentiometer"]
["EMC buil in","Version F","Version F"]
["Category Filter 3ph 380V ","C2 < 20 mt , C3 < 30 mt","C3 < 30 mt"]
["Category Filter 1ph 220V ","C2 < 20 mt , C3 < 30 mt","C2 < 20 mt , C3 < 30 mt"]
["Safety STO","Sil 2 Pl d (versione S)","Sil 2 Pl d (Versione S)"]
["Motor Type","IM, IPM/SPM ","IM, IPM/SPM "]
["Comunication Board","Modbus RTU Builtin","Modbus RTU Builtin"]
["CANOPEN ","Yes","Not available"]
["MODBUS TCP","Yes","Not available"]
["ETHERNET IP","Yes","Not available"]
["PROFIBUS DP","Yes","Not available"]
["PROFINET","Not available","Not available"]
["ETHERCAT","Yes","Not available"]
["PLC","Built-in","Not available"]
["Temperature ","-20°C + 50°C (-60°C Derating)","-20°C + 50°C (-60°C Derating)"]
["HMI","Remotable","Fixed"]